Frequency modification for FT-1900

|  |
| --- |
| * remove the 3 screws on the front panel(display)
* remove the display from the chasis.And take care for the flat cable.
* Find the 3 jumpers near the CPU.
* normally 1 and 2 are open and 3 in close.
* open 3. if 1 anf 2 are close open them.
* screw back the 3 screws
* press and hold DW/REV and A/N and MW and switch on the RADIO
* press D/MR ........and enjoy.

Jumper before modification.http://www.mods.dk/mod/_1/4455_ft-1900_before_modification.jpg |