FTM-400DR YAESU

|  |
| --- |
| New frequecy after the modification:136-174 mhz RX/TX400-480 mhz RX/TX1. Open the upper shell (speaker)
2. Lithium battery locate the left side
3. Identify positive symbol lithium battery
4. Remove resistance as photos

Perform as cpu reset page 61Picture: FTM-400-MOD2.JPGhttp://www.mods.dk/mod/_2/5130_FTM-400-MOD2_thumb.JPGPicture: ftm-400-mod1.JPGhttp://www.mods.dk/mod/_2/5130_ftm-400-mod1_thumb.JPG |