FTM-400DR YAESU

|  |
| --- |
| New frequecy after the modification: 136-174 mhz RX/TX 400-480 mhz RX/TX   1. Open the upper shell (speaker) 2. Lithium battery locate the left side 3. Identify positive symbol lithium battery 4. Remove resistance as photos   Perform as cpu reset page 61  Picture: FTM-400-MOD2.JPG [http://www.mods.dk/mod/_2/5130_FTM-400-MOD2_thumb.JPG](http://www.mods.dk/dl_article.php?Sub=2&File=5130_FTM-400-MOD2.JPG)  Picture: ftm-400-mod1.JPG [http://www.mods.dk/mod/_2/5130_ftm-400-mod1_thumb.JPG](http://www.mods.dk/dl_article.php?Sub=2&File=5130_ftm-400-mod1.JPG) |