Frequency modification for FT-1900

|  |
| --- |
| * remove the 3 screws on the front panel(display) * remove the display from the chasis.And take care for the flat cable. * Find the 3 jumpers near the CPU. * normally 1 and 2 are open and 3 in close. * open 3. if 1 anf 2 are close open them. * screw back the 3 screws * press and hold DW/REV and A/N and MW and switch on the RADIO * press D/MR ........and enjoy.   Jumper before modification. http://www.mods.dk/mod/_1/4455_ft-1900_before_modification.jpg |